# Technical Data

Cordless tacker |  | AdvancedTacker 18V-25
--- | --- | ---
Article number |  | ‎3 603 BA7 1..‎
Impact rate | min-1 | 30
Fasteners
Staple strip |  | Narrow crown staples
Bosch typeA) |  | TK 40
Width | mm | 5.8
Length | mm | 15 20 25
Nail strip |  | Brads
Bosch typeB) |  | SK 50
Head width | mm | 2.0
Length | mm | 16 19 25 30
Capacity (fasteners) |  | 100
WeightC) | kg | 2.1
Permitted ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationD) and during storage | °C | −20 to +50
Recommended rechargeable batteries |  | PBA 18V....W-.
Recommended battery chargersE) |  | AL 18…

A)

  Alternative staple types: Rapid Type 606, 12 mm, 15 mm, 18 mm, 23 mm, 25 mm

B)

  Alternative nail types: Rapid Type 8, 15 mm, 20 mm, 25 mm

C)

  Without rechargeable battery (you can find the battery weight at www.bosch-diy.com)

D)

  Limited performance at temperatures < 0 °C

E)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.