# Technical Data

Heat gun | EasyHeat 18V-500
--- | ---
Article number |  | ‎3 603 BA8 0..‎‎‎‎
Rated voltage | V | 18
Air volume standard settingA)B) | l/min | 100
Air volume boost settingA)B) | l/min | 120
Working temperature standard settingB) | °C | 350
Working temperature boost settingB) | °C | 450
Temperature in the nozzle outletB) | °C | 500
Temperature measurement accuracy | °C | ±75
WeightC) | kg | 0.5
Dimensions (length × width × height) | mm | 172 × 71 × 207
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationD) and during storage | °C | −20 to +50
Compatible rechargeable batteries |  | PBA 18V…W–.
Recommended rechargeable batteries |  | PBA 18V…W–. ≥ 4 Ah
Recommended chargersE) |  | AL 18...

A)

  The amount of air increases when the temperature rises from 350 °C to 450 °C. The speed of the fan is identical at both power settings.

B)

  At an ambient temperature of 20 °C and use of a rechargeable battery ≥ 4 Ah

C)

  Weight without battery

D)

  Limited performance at temperatures < 0 °C

E)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV