# Continuous light green battery charge indicator

×

A continuous light on the battery charge indicator (2) signals that the battery is fully charged or that the temperature of the battery is not within the permitted charging temperature range (0–45 °C), and can therefore not be charged. The battery is charged as soon as the permitted charging temperature range is reached.

When there is no battery inserted, the continuous light of the battery charge indicator (2) signals that the mains plug is plugged into the plug socket and that the charger is ready to be used.