# Technical Data

All-purpose saw | AdvancedCut 18
--- | ---
Article number |  | ‎3 603 CD5 1..‎‎‎‎
Rated voltage | V= | 18
No-load speed n₀A) | min−1 | 0−7000
Max. cutting depth | mm | 65
Weight according to EPTA‑Procedure 01:2014A) | kg | 1.1 (1.5 Ah)–1.4 (6.0 Ah)
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationB) and during storage | °C | −20 to +50
Recommended rechargeable batteries |  | PBA 18V…W-.
Recommended chargersC) |  | AL 18…

A)

  Depends on battery in use

B)

  Limited performance at temperatures < 0 °C

C)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV