# Working Advice

- Switch the power tool off immediately if the saw blade becomes blocked.

- Always use a sturdy support when working on small or thin workpieces.

- Make sure you always cut from front to back (see figure B) or from top to bottom (see figure C) when sawing.

To increase the cutting speed, saw in a gentle rocking motion (in the cutting direction).

Switch the power tool off immediately if the saw blade jams. Widen the sawing gap slightly with a suitable tool and pull the power tool out.

The riving knife (3) prevents sawing against the running direction of the chain saw (see figure D).

Put the cover (12) on the saw blade (1) after finishing work in order to protect it.