# Technical Data

Angle Grinder |  | UniversalGrind 750-115 | UniversalGrind 750-125 | UniversalGrind 7-125
--- | --- | --- | --- | ---
Article number |  | ‎3 603 CE2 0..‎ | ‎3 603 CE2 0..‎ | ‎3 603 CE2 0..‎
Rated power input | W | 750 | 750 | 750
Rated speedA) | min–1 | 12,000 | 12,000 | 12,000
Max. grinding disc diameter/rubber sanding pad diameter | mm | 115 | 125 | 125
Grinding spindle thread |  | M 14 | M 14 | M 14
Max. thread length of grinding spindle | mm | 11.5 | 11.5 | 11.5
Restart protection |  | ● | ● | ●
WeightB)C)
with standard auxiliary handle | kg | 1.9 | 1.9 | 1.9
Protection class |  | / II | / II | / II

A)

  Rated no-load speed for the selection of appropriate application tools in accordance with EN IEC 62841-2-3. The actual no-load speed is lower for safety reasons and according to production tolerances.

B)

  Weight without mains connection cable and without mains plug

C)

  Depends on protective guard ((5), (6), (7)) and auxiliary handle ((4)) in use

Angle Grinder |  | UniversalGrind 850-125 | UniversalGrind 8500-125
--- | --- | --- | ---
Article number |  | ‎3 603 CE2 1..‎ | ‎3 603 CE2 1..‎
Rated power input | W | 850 | 850
Rated speedA) | min–1 | 12,000 | 12,000
Max. grinding disc diameter/rubber sanding pad diameter | mm | 125 | 125
Grinding spindle thread |  | M 14 | M 14
Max. thread length of grinding spindle | mm | 11.5 | 11.5
Restart protection |  | ● | ●
WeightB)C)
with standard auxiliary handle | kg | 1.9 | 1.9
Protection class |  | / II | / II

A)

  Rated no-load speed for the selection of appropriate application tools in accordance with EN IEC 62841-2-3. The actual no-load speed is lower for safety reasons and according to production tolerances.

B)

  Weight without mains connection cable and without mains plug

C)

  Depends on protective guard ((5), (6), (7)) and auxiliary handle ((4)) in use

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.