# Technical Data

Angle grinder |  | AdvancedGrind 18V-80 | UniversalGrind 18V-75 | UniversalGrind 18V-75
--- | --- | --- | --- | ---
Article number |  | ‎3 603 CE5 100‎ | ‎3 603 CE5 000‎ | ‎3 603 CE5 001‎
Rated voltage | V= | 18 | 18 | 18
Rated no-load speedA)B) | min-1 | 12000 | 12000 | 12000
Speed adjustment range | min-1 | 2800–12,000 | – | –
Max. grinding disc diameter/rubber sanding pad diameter | mm | 125 | 115 | 125
Grinding spindle thread |  | M 14 | M 14 | M 14
Max. thread length of grinding spindle | mm | 21.7 | 21.7 | 21.7
Constant electronic control |  | ● | ● | ●
Speed preselection |  | ● | – | –
Soft start |  | ● | ● | ●
Restart protection |  | ● | ● | ●
Overload protection |  | ● | ● | ●
Weight according to EPTA-Procedure 01:2014C) | kg | 2.4 (6.0 Ah) | 2.3 (6.0 Ah) | 2.4 (6.0 Ah)
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35 | 0 to +35
Permitted ambient temperature during operationD) and during storage | °C | –5 to +50 | –5 to +50 | –5 to +50
Compatible rechargeable batteries |  | PBA 18V...W-. | PBA 18V...W-. | PBA 18V...W-.
Recommended rechargeable batteries for maximum performance |  | PBA 18V...W-. ≥ 4.0 Ah | PBA 18V...W-. ≥ 4.0 Ah | PBA 18V...W-. ≥ 4.0 Ah
Recommended battery chargersE) |  | AL 18... | AL 18... | AL 18...

A)

  Measured at 20–25 °C with rechargeable battery PBA 18V 6.0Ah.

B)

  Rated no-load speed for the selection of appropriate application tools in accordance with EN IEC 62841-2-3. The actual no-load speed is lower for safety reasons and according to production tolerances.

C)

  Depends on rechargeable battery, protective guard, and auxiliary handle in use

D)

  Limited performance at temperatures < 0 °C

E)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV