# Charging times

The following table displays the approximate time required in minutes in order to fully charge the battery, depending on the battery type. Charging times can vary. To find out more, visit: www.bosch-diy.com/wac

## AL 1810 CV

Rechargeable battery |
--- | ---
PBA 18V-1,5 Ah W-A | ≈ 83
PBA 18V-2,0 Ah W-B | ≈115
PBA 18V-2,5 Ah W-B | ≈136
PBA 18V-3,0 Ah W-B | ≈169
PBA 18V-3,0 Ah W-C | ≈172
PBA 18V-4,0 Ah W-C | ≈228
PBA 18V-4,0 Ah Power Plus | ≈219
PBA 18V-5,0 Ah W-C | ≈276
PBA 18V-6,0 Ah W-C | ≈335

## AL 18V-20

Rechargeable battery |
--- | ---
PBA 18V-1,5 Ah W-A | ≈49
PBA 18V-2,0 Ah W-B | ≈65
PBA 18V-2,5 Ah W-B | ≈80
PBA 18V-3,0 Ah W-B | ≈99
PBA 18V-3,0 Ah W-C | ≈95
PBA 18V-4,0 Ah W-C | ≈116
PBA 18V-4,0 Ah Power Plus | ≈123
PBA 18V-5,0 Ah W-C | ≈154
PBA 18V-6,0 Ah W-C | ≈188

corresponds to a full state of charge