# Practical Advice

Carry the cordless worklight by its handle (2).

The light head (1) becomes hot during operation. Let the cordless worklight cool down before adjusting it or transporting it.

Do not leave the cordless worklight unattended while it is switched on.

The cordless worklight will flash three times just before it is about to switch off due to an empty battery.

## Attaching the cordless worklight

You can use the hook (7) and the magnet (6) to attach the cordless worklight to suitable objects.

Always check the worklight is positioned on a stable surface/object and is not too close to heat-sensitive or flammable objects.

Avoid scratching delicate surfaces.

## Charging External USB Devices (see figure B)

- Ensure that your external USB device can be charged via the USB Type-C® port on the cordless worklight. Refer to the relevant specifications in the "Technical Data" section.

Connect the charging cable of your USB device to the USB Type-C® port (9). Press the USB button (3) of the cordless worklight to start the charging process.

The charging process is terminated as soon as a fully charged battery is detected. Disconnect the charging cable from the USB Type-C® port (9) to preserve the battery of the external USB device.