# Technical Data

Cordless worklight | EasySpotLight 18V-400
--- | ---
Article number |  | ‎3 603 JA1 200‎
Rated voltage | V= | 18
Rated power input | W | 4.5
Lighting duration, approx.A)B) | min/Ah | 310
Total luminous flux, max.B) | lm | 400
Recommended ambient temperature during charging | °C | 0 … +35
Permitted ambient temperature during operationC) and during storage | °C | −20 … +50
Recommended rechargeable batteries |  | PBA 18V…W-.D)
Recommended chargersE) |  | AL 18…D)
USB port |  | USB Type-C®
Output voltage | V | 5
Output current, max.F) | A | 1

A)

  At full brightness (excluding remaining operating time in dimmed mode)

B)

  Measured at 20–25 °C with rechargeable battery PBA 18V 2.0Ah.

C)

  Limited performance at temperatures < 0 °C

D)

  plus batteries and chargers for the POWER FOR ALL system

E)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV Professional, AL 1820 CV Professional, AL 1860 CV Professional, AL 2215 CV Professional

F)

  The actual output current depends on the USB device connected and its electricity demand.

The colour rendition of illuminated objects can be distorted.