# Starting Operation

With the battery inserted, the cordless worklight is ready to use.

##

Carefully unfold the handle/stand (5) and, if necessary, the hook (4) and position the cordless worklight. Ensure the cordless worklight is positioned on a stable surface/object and is not too close to heat-sensitive or flammable objects.

The lamp head (1) can be turned to different positions within the handle/stand (5).

##

Light switch (2) | Function
--- | ---
Press 1× | Switches on the cordless worklight, low brightness
Press 2× | Switches on the cordless worklight, medium brightness
Press 3× | Switches on the cordless worklight, full brightness
Press 4× | Switches off the cordless worklight
Press and hold | Switches off the cordless worklight

##

If the permissible operating temperature is exceeded, the cordless worklight switches itself off. To continue using the cordless worklight, let it cool down.