# Technical Data

Cordless worklight | UniversalWorkLight 18V-2100
--- | ---
Article number |  | ‎3 603 JA1 300‎
Rated voltage | V= | 18
Rated power input | W | 17
Lighting duration, approx.A)B) | min/Ah | 70
Total luminous flux, max.B) | lm | 2100
Recommended ambient temperature during charging | °C | 0 … +35
Permitted ambient temperature during operationC) and during storage | °C | –20 … +40
Recommended rechargeable batteries |  | PBA 18V…W-.D)
Recommended battery chargersE) |  | AL 18…D)

A)

  At full brightness (excluding remaining operating time in dimmed mode)

B)

  Measured at 20–25 °C with rechargeable battery PBA 18V 2.0Ah

C)

  Limited performance at temperatures < 0 °C

D)

  plus batteries and chargers for the POWER FOR ALL system

E)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV Professional, AL 1820 CV Professional, AL 1860 CV Professional, AL 2215 CV Professional

The colour rendition of illuminated objects can be distorted.