# Auxiliary handle

- Make sure that the auxiliary handle is always tightened. Otherwise you could lose control of the power tool when working.

## Swivelling the auxiliary handle (see figure A)

You can swivel the auxiliary handle (15) to any angle for a safe work posture that minimises fatigue.

- Loosen the wing bolt (14) of the auxiliary handle (15) and adjust the auxiliary handle (15) to the required position. Then retighten the wing bolt (14) of the auxiliary handle (15).
  Make sure that the clamping ring of the auxiliary handle slots into the corresponding groove on the housing.