# Technical Data

Cordless Drill/Driver |  | UniversalDrill 18V-60 | UniversalImpact 18V-60
--- | --- | --- | ---
Article number |  | ‎3 603 JD7 0..‎ | ‎3 603 JD7 1..‎
Rated voltage | V= | 18 | 18
No-load speedA)
First gear | min-1 | 0–500 | 0–500
Second gear | min-1 | 0–1900 | 0–1900
Max. torque, hard/soft screwdriving application according to ISO 5393A) | Nm | 47/24 | 42/24
Max. torqueA) | Nm | 60 | 60
Impact rate at no-load speedA) | min-1 | – | 0–28500
Max. drilling diameter (1st/2nd gear)
Masonry | mm | – | 13
Steel | mm | 13 | 13
Wood | mm | 35 | 35
Chuck capacity | mm | 13 | 13
Max. screw diameter | mm | 10 | 10
WeightB) | kg | 1.3 (1.5 Ah)–1.6 (6.0 Ah) | 1.3 (1.5 Ah)–1.6 (6.0 Ah)
Recommended ambient temperature during charging | °C | 0 ... +35 | 0 ... +35
Permitted ambient temperature during operationC) and during storage | °C | –20 ... +50 | –20 ... +50
Recommended rechargeable batteries |  | PBA 18V...W-. | PBA 18V...W-.
Recommended battery chargersD) |  | AL 18… | AL 18…

A)

  Measured at 20–25 °C with rechargeable battery PBA 18V 2.0Ah

B)

  Depending on battery in use

C)

  Limited performance at temperatures < 0 °C

D)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV Professional, AL 1820 CV Professional, AL 1860 CV Professional, AL 2215 CV Professional