# Technical Data

Cordless Drill/Driver |  | EasyDrill 18V-38 | EasyImpact 18V-38
--- | --- | --- | ---
Article number |  | ‎3 603 JD8 0..‎ | ‎3 603 JD8 1..‎
Rated voltage | V= | 18 | 18
No-load speedA)
First gear | min-1 | 0–430 | 0–430
Second gear | min-1 | 0–1630 | 0–1630
Max. torque, hard/soft screwdriving application according to ISO 5393A) | Nm | 36/19 | 36/19
Max. torqueA) | Nm | 38 | 38
Impact rate at no-load speedA) | min-1 | – | 0–24450
Max. drilling diameter (1st/2nd gear)
Masonry | mm | – | 10
Steel | mm | 10 | 10
Wood | mm | 30 | 30
Chuck capacity | mm | 10 | 10
Max. screw diameter | mm | 8 | 8
WeightB) | kg | 1.2 (1.5 Ah)–1.6 (6.0 Ah) | 1.3 (1.5 Ah)–1.6 (6.0 Ah)
Recommended ambient temperature during charging | °C | 0 ... +35 | 0 ... +35
Permitted ambient temperature during operationC) and during storage | °C | –20 ... +50 | –20 ... +50
Recommended rechargeable batteries |  | PBA 18V...W-. | PBA 18V...W-.
Recommended battery chargersD) |  | AL 18… | AL 18…

A)

  Measured at 20–25 °C with rechargeable battery PBA 18V 2.0Ah

B)

  Depending on battery in use

C)

  Limited performance at temperatures < 0 °C

D)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV Professional, AL 1820 CV Professional, AL 1860 CV Professional, AL 2215 CV Professional