# Starting Operation

##

The rotational direction switch (6) is used to change the rotational direction of the power tool. However, this is not possible while the on/off switch (5) is being pressed.

Clockwise: To drive in screws, press the rotational direction switch (6) all the way to the left.

Anti-clockwise: To loosen or unscrew screws, press the rotational direction switch (6) all the way to the right.

##

To start the power tool, press and hold the on/off switch (5).

The worklight (3) lights up when the on/off switch (5) is lightly or fully pressed, allowing the work area to be illuminated in poor lighting conditions.

To switch off the power tool, release the on/off switch (5).

##

The drill spindle, and therefore the tool holder, are locked when the on/off switch (5) is not pressed.

This allows screws to be driven in even when the battery is discharged and enables the power tool to be used as a screwdriver.

- If the drill spindle is blocked, do not press the on/off switch (5) for longer than 15 seconds. Otherwise, the power tool may become damaged.

##

- Only apply the power tool to the screw/nut when the tool is switched off. Rotating tool inserts can slip off.