# Technical Data

Cordless Screwdriver |  | IXO
--- | --- | ---
Article number |  | ‎3 603 JE0 0..‎‎‎‎
Rated voltage | V= | 3.6
No-load speed | min-1 | 0–235
Max. torque, hard/soft screwdriving application according to ISO 5393 | Nm | 5.5/3.0
Max. screw diameter | mm | 5
Weight | kg | 0.34
Recommended ambient temperature during charging | °C | 5 to +40
Charging voltage | V | 5
Max. charging current | mA | 1000
Permitted ambient temperature during operationA)B) and during storage | °C | –20 to +50
Rechargeable battery |  | Li-ion
Capacity | Ah | 2.0
Energy | Wh | 7.2
Number of battery cells |  | 1
Recommended power supply
Article number (5 V; 1000 mA) |  | ‎‎‎‎‎‎2 609 120 713 (EU) ‎‎‎‎‎‎‎ ‎‎2 609 120 718 (UK)‎‎‎‎‎‎‎‎‎‎
Max. charging time | h | 3
Protection class |  | /II
For additional technical data, visit: www.bosch-do-it.com/ecodesign
Recommended charging cable
Article number |  | 1 607 000 CG9 1 607 000 DN8

A)

  Overheat protection stops the power tool at temperatures > +65 °C.

B)

  Limited performance at temperatures < 0 °C