# Technical Data

Cordless fan | UniversalFan 18V-1000
--- | ---
Article number |  | 3 603 JE1 0..
Rated voltage | V= | 18
Max. airflow | m3/h | 1000
Speed | min−1 | 1500
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationA) | °C | 0 to +50
Permitted ambient temperature during storage (fan) |  | –20 to +70
Permitted ambient temperature during storage (rechargeable battery) |  | –20 to +50
Humidity operating range |  | Non-condensing
Weight according to EPTA-Procedure 01:2014B) |  | 2.7 kg (1.5 Ah) – 3.0 kg (6.0 Ah)
Dimensions (length x width x height) | mm | 254 x 310 x 414
Recommended rechargeable batteries |  | PBA 18V…W-.
Recommended battery chargersC) |  | AL 18...

A)

  Limited performance at temperatures < 10 °C

B)

  Depends on battery in use

C)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV