# Mounting the Fan

Note: The fan can be mounted in a vertical or horizontal position. Make sure that the fan is mounted such that fan operation is not impeded.

## Mounting on the Keyhole (see figure C)

Position the wide part of the keyhole (8) above the screw head (Ø 4 – 6 mm).

Push the fan downwards until the screw is in the narrow part of the keyhole and the fan is secured.

## Mounting on the Utility Hook (see figure D)

Fully pull the utility hooks (5) out of their slots.

Rotate the utility hooks if necessary.

Note: It is only possible to rotate the utility hooks when they are fully extended.

Mount the fan in a stable position (max. depth 36 mm).