# Technical Data

Cordless Drill/Driver |  | AdvancedDrill 18V-80 | AdvancedImpact 18V-80
--- | --- | --- | ---
Article number |  | ‎3 603 JE2 0..‎ | ‎3 603 JE2 1..‎
Rated voltage | V= | 18 | 18
No-load speedA)
Screwdriving (1st gear) | min-1 | 0–500 | 0–500
Drilling/impact drilling (2nd gear) | min-1 | 0–1950 | 0–1950
Impact rateA) | min-1 | – | 0–29250
Max. torque, hard/soft screwdriving application according to ISO 5393B) | Nm | 54/36 | 55/37
Max. torqueB) | Nm | 78 | 82
Max. drilling diameter (1st/2nd gear)
Masonry | mm | – | 13
Steel | mm | 13 | 13
Wood | mm | 40 | 40
Chuck capacity | mm | 13 | 13
Max. screw diameter | mm | 10 | 10
WeightC)D) | kg | 1.6 (1.5 Ah)–1.9 (6.0 Ah) | 1.7 (1.5 Ah)–2.0 (6.0 Ah)
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35
Permitted ambient temperature during operationE) and during storage | °C | –20 to +50 | –20 to +50
Recommended rechargeable batteries |  | PBA 18V...W-. | PBA 18V...W-.
Recommended chargersF) |  | AL 18... | AL 18...

A)

  Measured at 20–25 °C with rechargeable battery PBA 18V 6.0Ah

B)

  Measured at 20–25 °C without adapter, with rechargeable battery PBA 18V 6.0Ah.

C)

  Depends on battery in use

D)

  including drill chuck and handle

E)

  Limited performance at temperatures < 0 °C

F)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV