# Wall mounting

- Pull the plug out of the socket before carrying out any work on the charger.

The charger can be used either free-standing (for use on a desktop) or mounted on the wall.
When affixing to the wall: Use round-head screws with a diameter of 5 mm to max. 6.5 mm.

## AL 18V-44

Drill two holes, leaving a clearance of 56 mm.

## AL 2x18V-88

Drill two holes, leaving a clearance of 168 mm.