# Product Features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Keyless quick-change chuck (GBH 2-26 DFR)
(2) | SDS plus quick-change chuck (GBH 2-26 DFR)
(3) | SDS plus tool holder
(4) | Dust protection cap
(5) | Locking sleeve
(6) | Locking ring for quick-change chuck (GBH 2-26 DFR)
(7) | Rotational direction switch
(8) | Lock-on button for on/off switch
(9) | On/off switch
(10) | Release button for impact/mode selector switch (GBH 2-26 DRE, GBH 2-26 DFR)
(11) | Impact/mode selector switch (GBH 2-26 DRE, GBH 2-26 DFR)
(12) | Button for depth stop adjustment
(13) | Depth stop
(14) | Auxiliary handle (insulated gripping surface)
(15) | Release button for "drilling/hammer drilling" selector switch (GBH 2-26 RE)
(16) | "Drilling/hammer drilling" selector switch (GBH 2-26 RE)
(17) | Handle (insulated gripping surface)
(18) | Securing screw for keyed chuckA)
(19) | Keyed chuckA)
(20) | SDS plus shank for drill chuckA)
(21) | Drill chuck holder (GBH 2-26 DFR)
(22) | Front sleeve of the keyless quick-change chuck (GBH 2-26 DFR)
(23) | Retaining ring of the keyless quick-change chuck (GBH 2-26 DFR)
(24) | Dust extraction (GDE 16 Plus)A)
(25) | Dust collection capA)
(26) | Universal holder with SDS plus shankA)

A)

  This accessory is not part of the standard scope of delivery.