# Battery charge indicator

Note: Not all battery types have a battery charge indicator.

The green LEDs on the battery charge indicator indicate the state of charge of the battery. For safety reasons, it is only possible to check the state of charge when the power tool is not in operation.

Press the button for the battery charge indicator or to show the state of charge. This is also possible when the battery is removed.

If no LED lights up after pressing the button for the battery charge indicator, then the battery is defective and must be replaced.

The state of charge of the battery is also displayed on the user interface see Status indications.

## Battery model GBA 18V...

LED | Capacity
--- | ---
3× continuous green light | 60–100 %
2× continuous green light | 30–60 %
1× continuous green light | 5–30 %
1× flashing green light | 0–5 %

## Battery model ProCORE18V...

LED | Capacity
--- | ---
5 × continuous green light | 80–100 %
4 × continuous green light | 60–80 %
3 × continuous green light | 40–60 %
2 × continuous green light | 20–40 %
1 × continuous green light | 5–20 %
1 × flashing green light | 0–5 %