# Auxiliary handle

- Do not operate your power tool without the auxiliary handle (20).

- Make sure that the auxiliary handle is always tightened. Otherwise you could lose control of the power tool when working.

## Swivelling the auxiliary handle (see figure A)

You can swivel the auxiliary handle (20) to any angle for a safe work posture that minimises fatigue.

- Turn the lower gripping end of the auxiliary handle (20) anticlockwise and swivel the auxiliary handle (20) into the required position. Then turn the lower gripping end of the auxiliary handle (20) clockwise to retighten it.
  Make sure that the retaining strap of the auxiliary handle slots into the corresponding groove of the housing.