# Dust emission information

with GDE 18V-16

Dust emission values determined according to EN 50632-2-6:

Respirable dust: <0.5 mg/m3, K=0 mg/m3

Inhalable dust: <0.5 mg/m3, K=0 mg/m3

Quarz dust: < 0.05 mg/m3

The indicated dust emission value was determined under the following operating conditions:

Operating mode: Hammer drilling

Application tool: SDS plus drill bit, diameter 10 mm

Note: If the power tool is used in another operating mode, with other application tools or is poorly maintained, the dust emission value may differ. This may significantly increase dust emissions over the total working period.
If necessary, establish additional safety measures to protect the operator from the effects of dust emissions, for example: Wear a P2 filter class breathing mask.
The regulations on the material being machined that apply in the country of use must be observed.