# Battery is not being charged

## No battery is being charged and all six indicators (3) simultaneously flash red.

Cause: The charger has identified an internal error.

Corrective measure: Ensure that all batteries are fully inserted. Remove the mains plug and reinsert. If the error occurs again, have the charger checked by an authorised after-sales service centre for Bosch power tools.

## Battery is not being charged and the indicator (3) is flashing red (at the individual charging bay).

Cause: Battery is not correctly inserted.

Corrective measure: Insert the battery into the charger correctly.

Cause: The battery contacts and charging contacts are dirty.

Corrective measure: Clean the battery contacts and charging contacts; e.g. by inserting and removing the battery several times.

Cause: Battery defective

Corrective measure: Replace the battery.

## Battery is not being charged and the indicator (3) is lit up red.

Cause: Battery temperature is outside of the charging range

Corrective measure: Wait until the battery temperature is back within the permitted charging temperature range (0–45 °C).