# Charging times

The following table displays the approximate time required in minutes in order to reach the required state of charge, depending on the battery type and charging mode. The charging times can vary. Further information on this can be found at: www.bosch-professional.com/wac.

Rechargeable battery |  |
--- | --- | ---
GBA 18V 2.0 Ah | ≈17 | ≈29
GBA 18V 4.0 Ah | ≈23 | ≈37
GBA 18V 5.0 Ah | ≈28 | ≈47
ProCORE18V 4.0 Ah | ≈32 | ≈50
ProCORE18V 5.5 Ah | ≈29 | ≈47
ProCORE18V 8.0 Ah | ≈42 | ≈68
ProCORE18V 12.0 Ah | ≈65 | ≈96

corresponds to a state of charge of ≈ 80 %

corresponds to a full state of charge