# Technical Data

Battery adapter | UniversalUSB 18V-45
--- | ---
Article number |  | 1 600 A02 L3B 1 600 A02 L3C
USB port |  | 1x USB-A, 1x USB-C®A)
Output voltage | V= | 5
Max. output current B) Type C Type A | A | 3.0 1.5
Max. permitted length of USB cable | m | 1.5
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | PBA 18V...W-.
Recommended chargersD) |  | AL 18...

A)

  USB Type-C® and USB-C® are trademarks of USB Implementers Forum.

B)

  The actual output current (per USB port) depends on the USB device connected and its energy requirement.

C)

  Limited performance at temperatures < 0 °C

D)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV