# Charging times

The following table displays the approximate time required in minutes in order to reach the required state of charge, depending on the battery type and charging mode. The charging times can vary. Further information on this can be found at: www.bosch-professional.com/wac.

## Power Boost charging mode

The following charging times apply to one battery or two batteries that are charged simultaneously.

Rechargeable battery |  |
--- | --- | ---
2x EXBA18V-40 | ≈9 | ≈30
2x EXBA18V-55 | ≈11 | ≈31
2x EXBA18V-80 | ≈16 | ≈39
2x EXBA18V-150 | ≈27 | ≈60

corresponds to a state of charge of ≈ 50 %

corresponds to a full state of charge

## Standard charging mode

The following charging times apply to one battery or two batteries that are charged simultaneously.

Rechargeable battery |
--- | ---
2x EXBA18V-40 | ≈37
2x EXBA18V-55 | ≈35
2x EXBA18V-80 | ≈46
2x EXBA18V-150 | ≈60

corresponds to a full state of charge