# Technical Data

Battery Charger | EXAL18V2-320
--- | ---
Protection class | / II
Max. charging current (per charging bay) | 32 A (16 A)
Battery charging voltage (automatic voltage detection) | 18 V
WeightA) | 2.2 kg

A)

  Weight without mains connection cable and without mains plug

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.