# Mount the measuring tool on the rotating platform (see figure )

Place the measuring tool with the guide groove on the guide rail of the rotating platform and slide the measuring tool as far as it will go onto the platform.
To disconnect the measuring tool, pull it off the rotating platform in the opposite direction.

Roughly align the rotating platform horizontally using the height adjustment screws .