# Power supply

The inspection camera can be operated either with commercially available non-rechargeable batteries or with a Bosch lithium-ion rechargeable battery.

## Operation with battery adapter (see figure A)

The batteries are inserted into the battery adapter.

- The battery adapter is intended only for use in designated Bosch inspection cameras and must not be used with power tools.

To insert the non-rechargeable batteries, slide the cover (26) of the battery adapter into the port (28). Place the batteries into the cover as per the illustration on the cap (27). Slide the cap over the cover until you feel it click into place and it is flush with the handle of the inspection camera.

To remove the batteries, press the release buttons (18) on the cap (27) and pull the cap off. Pull out the cover (26) from inside the port (28).

Always replace all the batteries at the same time. Only use batteries from the same manufacturer and which have the same capacity.

- Remove the batteries from the inspection camera when not using it for longer periods. The batteries can corrode and self-discharge during prolonged storage.

## Operation with rechargeable battery (see figure B)

- Use only the chargers listed in the technical data. Only these battery chargers are matched to the lithium-ion batteries of your inspection camera.

Note: The use of rechargeable batteries unsuitable for your inspection camera can lead to malfunctions or damage to the inspection camera.

Note: The battery is supplied partially charged. To ensure full capacity of the battery, completely charge the battery before the first use.

The lithium-ion battery can be charged at any time without reducing its service life. Interrupting the charging process does not damage the battery.

To insert the charged rechargeable battery (17), slide it into the port (28) until you feel it click into place and it is flush with the handle of the inspection camera.

To remove the battery (17), press the release buttons (18) and pull it out of the port (28). Do not use force to do this.