# Operation

- Protect the handheld device and the rechargeable battery or battery adapter from direct sunlight. Protect the rechargeable battery or battery adapter against moisture. The camera cable (1) and camera head (4) are watertight if assembled correctly; the handheld device (15) is splash-proof. However, the rechargeable battery (16) and the battery adapter are not protected against water. If they come into contact with water, there is a risk of electric shock or damage.

- Do not use the inspection camera if the lens on the camera head (4) has fogged up. Switch the inspection camera on only if the moisture has evaporated. The inspection camera may otherwise become damaged.

- The switched-on light (5) can become hot during operation. To avoid burns, do not touch the light.

- Do not subject the inspection camera to extreme temperatures or variations in temperature. For example, do not leave it in a car for extended periods of time. In case of large variations in temperature, allow the inspection camera to adjust to the ambient temperature before putting it into operation.

Starting Operation
Main Menu
Saving/Transferring the Recordings
Saving/Transferring the Recordings
Working Advice