# Battery charge indicator

Note: Not all battery types have a battery charge indicator.

The green LEDs on the battery charge indicator indicate the state of charge of the rechargeable battery. For reasons of safety, it is only possible to query the state of charge when the cordless worklight is switched off.

Press the button for the battery charge indicator or to show the state of charge. This is also possible when the rechargeable battery is removed.

If no LED lights up after pressing the button for the battery charge indicator, then the rechargeable battery is defective and must be replaced.

## Battery model GBA 18V...

LED | Capacity
--- | ---
3× continuous green light | 60–100 %
2× continuous green light | 30–60 %
1× continuous green light | 5–30 %
1× flashing green light | 0–5 %

## Battery model ProCORE18V...

LED | Capacity
--- | ---
5 × continuous green light | 80–100 %
4 × continuous green light | 60–80 %
3 × continuous green light | 40–60 %
2 × continuous green light | 20–40 %
1 × continuous green light | 5–20 %
1 × flashing green light | 0–5 %