# Battery Charge Indicator on the Power Tool

The battery charge indicator on the power tool indicates the remaining battery capacity or an overload when the power tool is switched on.

LED | Capacity
--- | ---
3× continuous green light | 60–100 %
2× continuous green light | 30–60 %
1× continuous green light | 5–30 %
1× flashing green light | 0–5 %

LED | Meaning
--- | ---
Flashing light 3 × | Overload protection has been triggered
Flashing light middle LED | The temperature of the rechargeable battery is outside of the operating temperature range and/or the power tool's temperature protection has been triggered