# Status indicator (LED)

The following tables describes the LED status indicators (4) on the power tool.

Status indicator (LED) (4) | Meaning/cause | Solution
--- | --- | ---
Green | Status OK | –
Flashing red | Power tool has overheated and will switch off. | Leave the power tool to cool down. If the status indicator (LED) lights up green, the power tool can be switched on again.
Illuminated red | Kickback shutdown,restart protection or overload protection has been triggered, the power tool will switch off. | Turn the power tool off and on again.