# Operation

- Do not load the power tool so heavily that it comes to a stop.

- Before carrying out any work on the power tool (e.g. maintenance, tool change etc.), remove the battery from the power tool. There is risk of injury from unintentionally pressing the on/off switch.

- Exercise caution when cutting slots in structural walls; see the "Information on structural design" section.

- Clamp the workpiece if it is not secure under its own weight.

- If the power tool has been subjected to a heavy load, continue to run it at no-load for several minutes to cool down the accessory.

- Do not use the power tool with a cut-off stand.

- Do not touch grinding and cutting discs until they have cooled down. The discs can become very hot while working.

Working advice
Start-Up