# Safety Instructions for Saw Stands

- Disconnect the plug from the power source and/or remove the battery from the power tool before making any adjustments to the power tool or changing accessories. Accidents can occur when power tools are started unintentionally.

- Assemble the saw stand properly before mounting the power tool. Correct assembly is important to prevent the risk of collapsing.

- Firmly secure the power tool to the saw stand before using it. You may lose control of the power tool if it slips on the saw stand.

- Place the saw stand on a firm, flat, horizontal surface. If there is a chance that the saw stand will slip or wobble, the safe and steady machining of the workpiece cannot be guaranteed.

- Do not overload the saw stand or climb or stand on it. Overloading or standing on the saw stand can raise its centre of gravity, causing it to tip over.

- Do not force the workpiece into the saw blade. Exerting excessive pressure on the power tool can cause the saw stand to tip over.

- Ensure that all screws and connecting pieces are tightly fastened when carrying out work. Loose connections can cause instability and inaccurate sawing.

- Ensure that long and heavy workpieces do not unbalance the saw stand. The free end of long and heavy workpieces must have something placed underneath it or be supported.

- When pushing together or pulling apart the saw stand, do not put your fingers near the points of articulation. There is a risk of fingers being crushed.