# Battery charge indicator

The battery charge indicator indicates the remaining battery capacity or an overload for a few seconds when the power tool is switched on.

The battery charge indicator indicates the state of charge for a few seconds when the on/off switch is half or fully pressed.

LED | Capacity
--- | ---
3 × continuous green light | 75–100 %
2 × continuous green light | 40–75 %
1 × continuous green light | 15–40 %
1 × slowly flashing green light | 0–15 %

If the battery charge indicator flashes red, the power tool is overloaded.

The three LEDs in the battery charge indicator flash quickly when the temperature of the rechargeable battery is outside the operating temperature range and/or the overload protection has been triggered.