# Practical advice

The torque depends on the impact duration. The maximum achieved torque results from the sum of all individual torques achieved through impact. Maximum torque is achieved after an impact duration of 6–10 seconds. After this duration, the tightening torque increases only minimally.

## Tips for Changing Wheels

The power tool can be used for loosening and tightening wheel nuts and wheel bolts. When tightening, pay attention to the maximum tightening torque of the vehicle manufacturer in order to avoid damaging the screwed connection and to ensure a secure fit. Use a torque wrench to ensure that wheel screws and/or wheel nuts are tightened in accordance with the manufacturer's specifications.