# Battery Charge Indicator on the Cordless Worklight

The following information is displayed:

LED | Meaning
--- | ---
3 × continuous green light | State of charge ≈ 75–100 %
2 × continuous green light | State of charge ≈ 40–75 %
1 × continuous green light | State of charge ≈ 15–40 %
Flashing light outer LED | State of charge ≈ 0–15 %
Flashing light middle LED | Fault in the cordless worklight Contact Bosch customer services.
Flashing light all LEDs | Battery or cordless worklight outside the operating temperature Allow battery and cordless worklight to cool down.