# Battery charge indicator

The battery charge indicator indicates the state of charge for a few seconds when the on/off switch is half or fully pressed.

LED | Capacity
--- | ---
3 × continuous green light | 75–100 %
2 × continuous green light | 40–75 %
1 × continuous green light | 15–40 %
1 × slowly flashing green light | 0–15 %

The three LEDs in the battery charge indicator flash quickly when the overload protection has been triggered.If only the middle LED is flashing quickly, then the temperature of the rechargeable battery or the power tool is outside of the operating temperature range.Allow the battery and the power tool to cool.