# Battery Charge Indicator on the Power Tool

The battery charge indicator on the power tool indicates the state of charge for a few seconds when the on/off switch is half or fully pressed.

LED | State of charge
--- | ---
3 × continuous green light | ≈ 75–100 %
2 × continuous green light | ≈ 40–75 %
1 × continuous green light | ≈ 15–40 %
1 × slowly flashing green light | ≈ 0–15 %

The three LEDs in the battery charge indicator on the power tool flash quickly when the temperature of the rechargeable battery is outside the operating temperature range and/or the overload protection has been triggered.