# Status Indicator

##

The continuous green light on the status indicator (3) signals that there is no fault and the charger is ready for operation. If a battery is in the charging bay (1), the continuous green light on the status indicator (3) signals that the battery is being charged on the charger without any problems.

When the battery is fully charged, the status indicator (3) continues to light up green.

##

The continuous yellow light on the status indicator (3) indicates that the temperature of the battery is outside the permissible charging temperature range see Charging process.

As soon as the permissible charging temperature range is reached, the charging process begins and the status indicator switches to green.

##

The red continuous light/flashing light on the status indicator (3) signals an error on the battery or charger.