# Charging times

The following table displays the approximate time required in minutes in order to fully charge the battery, depending on the battery type. Charging times can vary. To find out more, visit: www.bosch-diy.com/wac

Rechargeable battery |
--- | ---
PBA 18V-1,5 Ah W-A | ≈ 30
PBA 18V-2,0 Ah W-B | ≈34
PBA 18V-2,5 Ah W-B | ≈43
PBA 18V-3,0 Ah W-B | ≈51
PBA 18V-3,0 Ah W-C | ≈45
PBA 18V-4,0 Ah W-C | ≈59
PBA 18V-4,0 Ah Power Plus | ≈65
PBA 18V-5,0 Ah W-C | ≈71
PBA 18V-6,0 Ah W-C | ≈87

corresponds to a full state of charge